IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2018-12-13T11:08:28"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20171027_0315(x64) - Exporter 17.4.0.0 - Alternate UI 17.4.0.0"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "AllenW" of Organization (no name given)
  Owner history of Person "AllenW" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 23.112487″ | longitude -0° 7′ 37.956022″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "London", "London", "United Kingdom"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 1 element
          1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "A40" | object type "A40" | names: "NBS_AndersonGECLtd_Snks_SeriesA_Single:A40:307206" | material: "NBS_Concept" | property sets: COBie

Types
  IFCSANITARYTERMINALTYPE "A40" | SINK | 1 occurrence | material: "NBS_Concept" | property sets: BOS_General, NBS_Data, Pset_SanitaryTerminalTypeSink, IFC, COBie

Property sets
  COBie | properties | on 1 object (1 IFCFLOWTERMINAL)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_40_20_96_81:Sinks" (IFCTEXT)
    CodePerformance = "EN 1.4301" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Single bowled stainless steel sink" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "30 years" (IFCTEXT)
    Features = "Can be integrated with stainless steel worktops, basket strainer waste and , overflow fittings included" (IFCTEXT)
    Finish = "Bright satin" (IFCTEXT)
    Grade = "EN 1.4301" (IFCTEXT)
    Manufacturer = "info@gecanderson.co.uk" (IFCTEXT)
    Material = "Stainless steel" (IFCTEXT)
    ModelNumber = "A40" (IFCTEXT)
    ModelReference = "A40" (IFCTEXT)
    Name = "Sinks_A40_AndersonGECLtd" (IFCTEXT)
    NominalHeight = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "440 x 440 x 200 mm" (IFCTEXT)
    SustainabilityPerformance = "100% Recyclable" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_AndersonGECLtd_Sinks_A40" (IFCTEXT)
    ManufacturerName = "Anderson, GEC Ltd" (IFCTEXT)
    ManufacturerURL = "www.gecanderson.co.uk" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/zpamyoxa" (IFCTEXT)
    NBSDescription = "Sinks" (IFCTEXT)
    NBSReference = "45-35-70/344" (IFCTEXT)
    ProductInformation = "http://www.gecanderson.co.uk/product/individual-bowls/a-series/index.html" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_40_20_96_81" (IFCTEXT)
    Uniclass2015Title = "Sinks" (IFCTEXT)
    Uniclass2015Version = "Products v1.11" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    FixingOptions = "Inset, undermount, flushmount" (IFCTEXT)
    FlatFlange = "20 mm with corner radius of 10 mm" (IFCTEXT)
    Form = "Single bowled sink" (IFCTEXT)
    Partition = "n/a" (IFCTEXT)
  Pset_SanitaryTerminalTypeSink | properties | on 1 type object
    Color = "n/a" (IFCTEXT)
    Mounting = "Inset, undermount, flushmount" (IFCTEXT)
    SinkType = "Other" (IFCTEXT)
  IFC | properties | on 1 type object
    IfcExportAs = "IfcSanitaryTerminalType" (IFCTEXT)
    IfcExportType = "SINK" (IFCTEXT)